|  |  |  |
| --- | --- | --- |
| **Comparison between M4 Mini and Our Customized Product** | | |
| **Topics** | **M4 Mini** | **Our Product** |
| Network Bonding: | 4 SIM & 1 Ethernet | 3 SIM & 1 Ethernet |
| Network Provided: | Wi-Fi | Wi-Fi (30 Meters Range) |
| Outdoor Work Duration: | 5-6 Hours | 8 Hours |
| Support Self-Built Server: | Linus Debain 9.0 OS Required | Linus Debain 9.0 OS Required |

|  |  |
| --- | --- |
| **Model** | **M4 Mini** |
| Cellular Network Mode | TDD-LTE, FDD-LTE, DC-HSPA+/HSPA+/HSPA/UMT, STD-SCDMA |
| Node Bands | Based on region |
| Lan Rate | 1000Mb/s |
| Wan Rate | 1000Mb/s |
| Wi-Fi Frequency | 2.4GHz, 5.8 GHz |
| Wi-Fi | 802.11b/g/n 300 Mb/s |
| Wi-Fi Range | 30 meters |
| Antena | External |
| Uplink Speed | 80Mb/s Max |
| Downlink Speed | 80Mb/s Max |
| Protocol | TCP/IP, UDP. FTP, HTTP |
| Support Daisy Chain | Yes |
| Management | Web Control |
| Battery Capacity | 9600 MA (built-in) |
| Working Duratrion | 5-6 hours / 8 hours |
| Power Supply | 12V 3A |
| Power Consumption | 5W |
| Server Binding Option | 1. Customer Rent Local Server 2. Mine Help Build Customer Own Server |
| Storage Temparature | -400C~700C |
| Working Temparature | -100C~400C |
| Storage Humidity | 5%-90% no condensation |
| Working Humadity | 10%-90% no condensation |